For 1990-2009 cars

## Console Trim Plate Replacement Automatic

### Removal Procedure

1. Use a flat blade tool in order to unsnap the accessory trim plate.
2. Disconnect the electrical connectors, if applicable.

### Installation Procedure

1. Connect the electrical connectors, if applicable.
2. Snap the accessory trim plate into place.

## Console Trim Plate Replacement Alero - Manual Transaxle

### Removal Procedure

1. Unsnap the shift boot fastener.
2. Use a flat blade tool in order to unsanap the accessory trim plate.
3. Disconnect the electrical connector for the ETS switch.
4. Compress the ETS retainers to remove it from the trim panel.

### Installation Procedure

1. Snap the ETS switch into place.
2. Push the trim plate into place.
3. Snap the shift boot retainer into place.