For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
2. Remove the rear seat belt latch anchor nut (2).
3. Remove the rear seat belt latch (1).

### Installation Procedure

1. Install the rear seat belt latch (1).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the rear seat belt latch nut (2).

Tighten
Tighten the bolt to 50 N·m (37 lb ft).

3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.