For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. For front doors refer to Front Side Door Trim Panel Replacement . For rear doors refer to Rear Side Door Trim Panel Replacement .
2. Remove the bolt (2) which secures the inside handle (1).
3. Remove the inside handle rod (4) from the inside handle (3).
4. Remove the door lock rod (2). from the inside handle (3).
5. Remove the inside door handle (3).

### Installation Procedure

1. Install the inside handle rod (4). to the inside handle (3).
2. Install the door lock rod (2). to the inside handle (3).
3. Install the inside door handle (3) to the door.
4. Install the inside handle bolt (2).
5. Install the door trim panel. For front doors refer to Front Side Door Trim Panel Replacement For rear doors refer to Rear Side Door Trim Panel Replacement .