For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Disconnect the positive battery cable.
3. Remove the battery hold down retainer.

Important: Do not tip the battery more than 40 degrees during removal.

4. Remove the battery.

### Installation Procedure

Important: Do not tip the battery more than 40 degrees during battery installation.

1. Install the battery to the battery tray.
2. Install the battery hold down retainer.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Connect the positive battery cable.

Tighten
Tighten the cable bolt to 15 N·m (11 lb ft).

4. Connect the negative battery cable bolt. Refer to Battery Negative Cable Disconnection and Connection .