For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the left front fender liner. Refer to Front Fender Liner Replacement in Body Front End.
3. Disconnect the washer hose from the washer pump.
4. Lower the vehicle.
5. Disconnect the washer hose from the left front fender.
6. Disconnect the washer hose from the wiper arms.
7. Disconnect the washer hose from the air inlet grille panel.
8. Remove the washer hose from the vehicle.

### Installation Procedure

1. Position the washer hose to the vehicle.
2. Connect the washer hose to the air inlet grille panel.
3. Connect the washer hose to the wiper arms.
4. Route the washer hose pump end down between the battery and the radiator core support to the washer pump.
5. Connect the washer hose to the left front fender.
6. Raise the vehicle.
7. Connect the washer hose to the washer pump.
8. Install the left front fender liner. Refer to Front Fender Liner Replacement in Body Front End.