For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the stabilizer shaft link. Refer to Stabilizer Shaft Link Replacement .
4. Remove the ABS harness from the lower control arm.
5. Remove the ball joint from the knuckle. Refer to Lower Control Arm Ball Joint Replacement .
6. Remove the bolt (2) attaching the control arm (1) to the front suspension crossmember (4).
7. Remove the bolt (3) from the control arm (1).
8. Remove the control arm (1) from the vehicle.

### Installation Procedure

1. Install the control arm (1) into position and install the bolt (2) attaching the control arm (1) to the crossmember (4).

Hand tighten the bolt.

2. Install the bolt (3) to the control arm (1).

Hand tighten the bolt.

3. Install the lower ball joint to the steering knuckle. Refer to Lower Control Arm Ball Joint Replacement .
4. Install the stabilizer shaft link. Refer to Stabilizer Shaft Link Replacement .
5. Install the ABS harness onto the lower control arm.
6. Slightly raise the vehicle.
7. Remove the jack stands from under the crossmember.
8. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

9. With the vehicle at curb height, tighten the control arm attaching bolts.

Tighten

• | Tighten the front suspension crossmember front bolt (3) to 60 N·m (45 lb ft) plus 120 degrees rotation.

• | Tighten the front suspension crossmember rear bolt (2) to 100 N·m (74 lb ft) plus 180 degrees rotation.

10. Check the front wheel alignment. Refer to Wheel Alignment Specifications .