For 1990-2009 cars

### Removal Procedure

1. Remove the push-pin retainer from the front of the rear fascia to the quarter panel.
2. Remove the retaining screws from the front of the rear fascia.
3. Remove the screws which secure the quarter panel to the front support bracket.
4. Pull back the fascia and remove the front support bracket.

### Installation Procedure

1. Position the front support bracket to the quarter panel.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the front support bracket to quarter panel screws.

Tighten
Tighten the front support bracket to quarter panel screws to 6 N·m (53 lb in).

3. Install the rear fascia to front support bracket screws.

Tighten
Tighten the rear fascia to front support bracket screws to 6 N·m (53 lb in).

4. Install the push-pin retainer to the front of the rear fascia to the quarter panel.