For 1990-2009 cars

### Removal Procedure

1. Disconnect the electrical connector at EGR valve.
2. Remove the 2 EGR Valve retaining nuts.
3. Remove the Linear EGR valve assembly.
4. Remove the gasket.

### Installation Procedure

1. Clean the intake surface and install the gasket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the linear EGR valve assembly and two bolts.

Tighten
Tighten the nuts to 30 N·m (22 lb. ft.).

3. Connect the electrical connector.