For 1990-2009 cars

### Removal Procedure

1. Open and support the door.
2. Remove the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Remove the rear door water deflector. Refer to Front Side Door Water Deflector Replacement .
4. Remove the rear door inside handle. Refer to Door Inside Handle Replacement .
5. Remove the rear door window regulator. Refer to Rear Side Door Window Regulator Replacement .
6. Remove the rear door energy absorber. Refer to Rear Door Energy Absorber Pad Replacement .
7. Remove the rear door outside handle. Refer to Rear Side Door Outside Handle Replacement .
8. Remove the rear door lock. Refer to Door Lock Replacement .
9. Remove the rear door window. Refer to Rear Side Door Window Replacement .
10. Remove the rear door stationary window. Refer to Rear Side Door Stationary Window Replacement .
11. Remove the rear door reveal molding. Refer to Rear Side Door Window Reveal Molding Replacement .
12. Remove the rear door rubber condiuit. Refer to Rear Side Door Conduit Replacement .
13. Remove the rear door electrical harness.
14. Remove the rear door check link. Refer to Door Check Link Replacement .
15. Remove the rear door hinges (3). Refer to Rear Side Door Hinge Replacement .
16. Remove the rear door from the body.

### Installation Procedure

1. Install the rear door hinges (3). Refer to Rear Side Door Hinge Replacement .
2. Install the rear door check link. Refer to Door Check Link Replacement .
3. Install the rear door electrical harness.
4. Install the rear door rubber condiuit. Refer to Rear Side Door Conduit Replacement .
5. Install the rear door reveal molding. Refer to Rear Side Door Window Reveal Molding Replacement .
6. Install the rear door stationary window. Refer to Rear Side Door Stationary Window Replacement .
7. Install the rear door window. Refer to Rear Side Door Window Replacement .
8. Install the rear door lock. Refer to Door Lock Replacement .
9. Install the rear door outside handle. Refer to Rear Side Door Outside Handle Replacement .
10. Install the rear door energy absorber. Refer to Rear Door Energy Absorber Pad Replacement .
11. Install the rear door window regulator. Refer to Rear Side Door Window Regulator Replacement .
12. Install the rear door inside handle. Refer to Door Inside Handle Replacement .
13. Install the rear door water deflector. Refer to Front Side Door Water Deflector Replacement .
14. Install the rear door trim panel. Refer to Rear Side Door Trim Panel Replacement .
15. Inspect the rear door for proper alignment.