For 1990-2009 cars

## Front Side Door Window Switch Replacement - Left Side Pontiac

### Removal Procedure

1. With a flat-bladed tool, push in and lift up to disengage the retaining clips (2) for the accessory trim plate (1).
2. Disconnect the electrical connector from the power window switch.
3. Release the power window switch retainers.
4. Remove the power window switch from the switch plate.

### Installation Procedure

1. Install the power window switch to the switch plate.
2. Press the power window switch into the switch plate until fully seated.
3. Connect the electrical connector to the power window switch.
4. Install the switch plate (1) to the door trim panel. Press the switch plate (1) into the trim panel until the retaining clips (2) are fully engaged.

## Front Side Door Window Switch Replacement - Left Side Oldsmobile

### Removal Procedure

1. Using a small flat-bladed tool, at the front of the switch, push in and lift up to release the front clip.
2. Remove the switch bezel from the door trim panel.
3. Disconnect the electrical connector from the power window switch.
4. Release the power window switch retainers in order to remove the switch from the bezel (1).

### Installation Procedure

1. Install the power window switch to the bezel (1), pressing into place until fully seated.
2. Connect the electrical connector to the power window switch.
3. Install the front door switch bezel (1) to the door trim panel, pressing into place until fully seated.