For 1990-2009 cars

Checks | Action
--- | ---
DEFINITION: A shudder or vibration occurs when accelerating the vehicle.
There is an excessive CV joint angle. | Repair the CV joint angle.
There is a sticking spider assembly (inner CV joint). | Lubricate or replace the inner CV joint. Refer to Wheel Drive Shaft Inner Joint and Boot Replacement .
There is a sticking joint assembly (outer CV joint). | Lubricate or replace the outer CV joint. Refer to Wheel Drive Shaft Outer Joint and Boot Replacement .