For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the hood side bumper (1), by pulling upward.
3. Remove the hood adjust front bumper (1), by pulling upward.

### Installation Procedure

1. Install the hood adjust front bumper (1).

Ensure the unit is retained.

2. Install the hood side bumper (1).

Ensure the unit is retained.

3. Adjust the hood adjust front bumper for the correct flushness between the hood and the front fender. Refer to Hood Adjustment .