For 1990-2009 cars

### Removal Procedure

Caution: Remove the fuel tank cap and relieve the fuel system pressure before servicing the fuel system in order to reduce the risk of personal injury. After you relieve the fuel system pressure, a small amount of fuel may be released when servicing the fuel lines, the fuel injection pump, or the connections. In order to reduce the risk of personal injury, cover the fuel system components with a shop towel before disconnection. This will catch any fuel that may leak out. Place the towel in an approved container when the disconnection is complete.

Caution: Wear safety glasses when using compressed air in order to prevent eye injury.

Caution: Place a dry chemical (Class B) fire extinguisher nearby before performing any on-vehicle service procedures. Failure to follow these precautions may result in personal injury.

Notice: Cap the fittings and plug the holes when servicing the fuel system in order to prevent dirt and other contaminants from entering the open pipes and passages.

Important: Always maintain cleanliness when servicing fuel system components.

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .
2. Grasp both sides of the quick-connect fitting. Twist quick-connect fitting ¼ turn in each direction to loosen any dirt within fitting.
3. Repeat for other fuel pipe fitting.
4. Using compressed air blow out dirt from the quick-connect fittings at both ends.
5. Squeeze plastic tabs of male end connector.
6. Pull connection apart.

Repeat for the other fitting.

7. Using a clean shop towel wipe off the male pipe end .
8. Clean or replace components/assemblies as required.

### Installation Procedure

Caution: Always apply a few drops of clean engine oil to the male pipe ends before connecting the fuel pipe fittings in order to reduce the risk of fire and personal injury. This will ensure proper reconnection and prevent a possible fuel leak. During normal operation, the O-rings located in the female connector will swell and may prevent proper reconnection if not lubricated.

1. Apply a few drops of clean oil to the male pipe end.
2. Push both sides of the quick-connect fitting together in order to cause the retaining tabs/fingers to snap into place.
3. Pull on both sides of the quick connect fitting in order to make sure the connection is secure.
4. Tighten the fuel filler cap.
5. Reconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
6. Inspect for fuel leaks.

6.1. | Turn ON the ignition for 2 seconds.

6.2. | Turn OFF the ignition for 10 seconds.

6.3. | Turn ON the ignition.

6.4. | Inspect for leaks.