For 1990-2009 cars

## Front Side Door Window Switch Replacement - Right Side Oldsmobile

### Removal Procedure

1. Remove the lower pull cup from the door trim panel. Refer to Armrest Pull Cup Replacement .
2. With a flat-bladed tool, push in and lift up to release the retaining clips for the accessory switch plate.
3. Disconnect the electrical connector from the power window switch.
4. Release the power window switch retainers. Push the switch out of the switch plate.

### Installation Procedure

1. Install the power window switch to the switch plate. Press the switch into the switch plate until fully seated.
2. Connect the electrical connector to the power window switch.
3. Install the switch plate into the door trim panel. Press the switch plate into the trim panel until the retaining clips are fully engaged.
4. Install the lower pull cup to the door trim panel. Refer to Armrest Pull Cup Replacement .

## Front Side Door Window Switch Replacement - Right Side Pontiac

### Removal Procedure

1. With a flat-bladed tool, push in and lift up to disengage the retaining clips for the accessory switch plate.
2. Disconnect the electrical connector from the power window switch.
3. Release the power window switch retainers.
4. Remove the power window switch from the switch plate.

### Installation Procedure

1. Install the power window switch to the switch plate.
2. Press the power window switch into the switch plate until fully seated.
3. Connect the electrical connector to the power window switch.
4. Install the switch plate to the door trim panel. Press the switch plate into the trim panel until the retaining clips are fully engaged.