For 1990-2009 cars

### Removal Procedure

1. Remove the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .
2. Remove the center pillar upper trim panel (1).

Pry outward to release the retainers.

### Installation Procedure

1. Install the center pillar upper trim panel (1).

Ensure the retainers lock into place.

2. Install the center pillar lower trim panel. Refer to Center Pillar Lower Trim Panel Replacement .