For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Access Cover Plate Nuts | 10 N·m | 89 lb in
Armrest Bracket Screws | 10 N·m | 89 lb in
Door Check Link to Door Nut | 10 N·m | 89 lb in
Door Check Link to Pillar Bolt | 9 N·m | 80 lb in
Door Handle Bezel Screw | 2 N·m | 18 lb in
Door Hinge Bolts | 28 N·m | 21 lb ft
Door Inside Handle Bolt | 10 N·m | 89 lb in
Door Intermedidate Hinge Bolt | 25 N·m | 18 lb ft
Door Locating Pin Bolt | 10 N·m | 89 lb in
Door Lock Actuator Screw | 6 N·m | 53 lb in
Door Lock Screws | 10 N·m | 89 lb in
Door Lock Striker Bolt | 25 N·m | 18 lb ft
Door Trim Panel Screw | 10 N·m | 89 lb in
Energy Absorber Nuts | 6 N·m | 53 lb in
Energy Absorber Strap Bolt | 6 N·m | 53 lb in
Front Door Locking System Module Bolt | 10 N·m | 89 lb in
Front Door Locking System Module Nut | 10 N·m | 89 lb in
Front Door Window Front Run Channel Lower Bolt | 10 N·m | 89 lb in
Front Door Window Front Run Channel Upper Screw | 1.5 N·m | 13 lb in
Front Door Window Rear Run Channel Bolt | 6 N·m | 53 lb in
Lower Switch Bezel Trim Panel Screws | 10 N·m | 89 lb in
Outside Door Handle Nut | 10 N·m | 89 lb in
Outside Rearview Mirror Nut | 10 N·m | 89 lb in
Power Window Motor Retaining Bolts | 6 N·m | 53 lb in
Rear Door Inside Handle Bolt | 10 N·m | 89 lb in
Rear Door Stationary Window to Inner Door Panel Bolt | 10 N·m | 89 lb in
Rear Door Stationary Window to Inner Door Panel Screw | 1.5 N·m | 13 lb in
Rear Door Window Channel Lower Bolt | 9 N·m | 80 lb in
Regulator Bolts | 10 N·m | 89 lb in
Regulator Cover Plate Nuts | 10 N·m | 89 lb in
Reveal Molding Screws | 6 N·m | 53 lb in
Rubber Seal Strip to Upper Window Frame Screw | 1.5 N·m | 13 lb in
Window Regulator Bolts | 10 N·m | 89 lb in
Window to Regulator Bolts | 10 N·m | 89 lb in