For 1990-2009 cars

### Removal Procedure

1. Release the front floor console power accessory port housing from the front floor console by using a small flat-bladed tool to release the retainer.
2. Remove the front floor console power accessory port housing from the front floor console.
3. Release the electrical connector retainer tabs from the power accessory port.
4. Disconnect the electrical connector from the power accessory port.
5. Remove the power accessory port element retainer.
6. Remove the power accessory port element.

### Installation Procedure

1. Align the power accessory port socket to the power accessory port housing.
2. Install the power accessory port element retainer.
3. Connect the electrical connector to the power accessory port.
4. Position the power accessory port housing to the front floor console.
5. Install the power accessory port housing into the front floor console pressing into place until fully seated.
6. Inspect the power accessory port for proper operation.