For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner Bracket Bolts | 10 N·m | 89 lb in
Battery Tray Screws | 5 N·m | 44 lb in
Bracket to Strut Tower Bolts | 10 N·m | 89 lb in
Fender Liner Bolts | 2 N·m | 18 lb in
Front Fender Front Brace Bolt | 10 N·m | 89 lb in
Front Fender Lower Bolts | 9 N·m | 80 lb in
Front Fender Rear Brace Bolt | 10 N·m | 89 lb in
Front Fender Rear Center Bracket to Front Fender Bolt | 10 N·m | 89 lb in
Front Fender Upper Bolts | 9 N·m | 80 lb in
Hood Hinge to Fender Bolts | 28 N·m | 21 lb ft
Hood Hinge to Hood Bolts | 25 N·m | 18 lb ft
Hood Latch Bolts | 10 N·m | 89 lb in
Hood Latch Release Cable Handle Screw | 3 N·m | 27 lb in
Hood Latch Striker Bolts | 25 N·m | 18 lb ft
Hood Latch Support Bolts | 25 N·m | 18 lb ft
Hood Latch Support Nuts | 25 N·m | 18 lb ft
Hood Release Handle Base Bolts | 2 N·m | 18 lb in