For 1990-2009 cars

### Removal Procedure

1. Raise the front floor console armrest.
2. Remove the screws from the front floor console armrest hinge.
3. Remove the front floor console armrest from the front floor console.

### Installation Procedure

1. Install the front floor console armrest to the armrest hinge.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the screws to the front floor console armrest hinge.

Tighten
Tighten the front floor console armrest hinge screws to 2 N·m (18 lb in).

3. Lower the lower front floor console armrest.