For 1990-2009 cars

Problem | Action
--- | ---
A misaligned column | Adujst the alignment as necessary. Adjust, repair and/or replace the following components as necessary:

• | The bearings

• | The mounting

Refer to Steering Column Replacement .

Loose column to steering gear joints | Inspect for the correct torque. Tighten the joints as necessary. Replace the components as needed Refer to Steering Column Replacement .
A worn or broken lower or upper steering shaft bearing | Replace the bearings as necessary. Refer to Steering Column Replacement .