For 1990-2009 cars

The brake system uses a single red BRAKE warning lamp located in the instrument panel cluster. When the ignition switch is in the START position, the BRAKE warning lamp turns ON. The warning lamp turns OFF when the ignition switch returns to the RUN position. The following conditions activate the BRAKE warning lamp:

• | The parking brake is applied. The lamp should be ON when the parking brake is applied and the ignition switch is ON.

• | The fluid level sensor detects a low fluid level. Refer to Master Cylinder Description .