For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Starting at the top, pull downward on the water deflector (1) in order to remove from the door edges.
3. Feed the electrical connectors (and inside handle rod) through the existing holes in the water deflector.

### Installation Procedure

1. Connect the electrical connectors (and inside handle rod) through the water deflector.
2. Install the water deflector (1) to the door.
3. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement