For 1990-2009 cars

## Emblem/Nameplate Replacement Alero

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. In order to remove an emblem/nameplate, heat the emblem/nameplate using J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool in order to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07502 or equivalent.

• | For plastic panels use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint-free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. If the location of the nameplate has not been marked, apply tape and use the following dimensions.

• | Dimension A is 203 mm (8.0 in) from the top left edge of the applique.

• | Dimension B is 32 mm (1.25 in) from the top edge of the applique.

4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement Grand Am

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07502 or equivalent.

• | For plastic panels use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (A) 139.6 mm (5 1/2 inches) from the top of the molding to the bottom of the emblem/name plate.

• | Dimension (B) 9.5 mm (3/8 inches) from the front edge of the door to the beginning of the emblem/name plate.

• | Dimension (C) 24 mm (15/16 inches) from the front edge of the door to the beginning of the emblem/name plate.

4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement Grand Am Emblem Front

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels, use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07501 or equivalent.

• | For plastic panels, use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. The Pontiac emblem is located in the relief of the front fascia.
4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement Alero Emblem Front

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels, use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07501 or equivalent.

• | For plastic panels, use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. The Oldsmobile emblem is located in the relief of the front fascia.
4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement Grand Am SE, Front Door

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07502 or equivalent.

• | For plastic panels use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (A) 102 mm (4.0 in) from the front edge of the door to the letter G.

• | Dimension (B) 7 mm (1/4 in) is the distance between Grand and Am.

• | Dimension (C) 29 mm (1 1/8 in) is the distance between Am and Se.

• | Dimension (D) 29 mm (1 1/8 in) is the distance from the door molding to the bottom edge of the emblem/name plate.

4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement Grand Am GT, Front Door

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07502 or equivalent.

• | For plastic panels use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (A) 120 mm (4 3/4 in) from the front edge of the door to the emblem.

• | Dimension (B) 8 mm (5/16 in) is the distance between the GRAND and the AM.

• | Dimension (C) 10 mm (13/32 in) is the distance between GRAND AM and GT.

• | Dimension (D) 24 mm (1 in) is the distance between molding and the emblem.

4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement Grand Am GT, Deck Lid

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07502 or equivalent.

• | For plastic panels use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (A) 29 mm (1 1/8 in) from the front edge of the deck lid to the letter T.

• | Dimension (B) 24 mm (1 in) is the distance from the deck lid to the bottom edge of the emblem.

• | Dimension (C) 8 mm (5/16 in) is the distance between Am and GT.

• | Dimension (D) 6 mm (1/4 in) is the distance between Grand and Am.

4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement Grand AM, Deck Lid

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07502 or equivalent.

• | For plastic panels use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (A) and (B) are equal. The emblem is centered on the key cylinder.

• | Dimension (D) 10 mm (13/32 in) is the distance between Grand and Am.

• | Dimension (C) 23 mm (15/16 in) is the distance from the deck lid to the bottom edge of the emblem/name plate.

4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement V6 Fender

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07502 or equivalent.

• | For plastic panels use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (A) 95 mm (3 3/4 in) from the front edge headlamp seal to the emblem.

• | Dimension (B) 21 mm (13/16 in) is the distance bottom edge of the fender and the emblem.

4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement V6HO Fender

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07502 or equivalent.

• | For plastic panels use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | Dimension (A) 70 mm (2 3/4 in) from the front edge headlamp seal to the emblem.

• | Dimension (B) 28 mm (1 1/8 in) is the distance bottom edge of the fender and the emblem.

4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.

## Emblem/Nameplate Replacement Deck Lid Emblem

#### Tools Required

J 25070 Heat Gun

### Removal Procedure

1. When replacing or repairing an emblem/nameplate do the following:

1.1. | Use tape to protect the mounting surface during removal.

1.2. | Use tape for alignment marks for installation of the emblem/nameplate.

2. To remove an emblem/nameplate, heat the emblem/nameplate using a J 25070 .

Apply heat using a circular motion for about 30 seconds.

Notice: Use a plastic, flat-bladed tool to prevent paint damage when removing an emblem/name plate.

3. Use a plastic, flat-bladed tool to lift or remove the emblem/nameplate from the panel surface.

Important: If tape is still intact on the molding or panel, do not remove the tape. Clean the tape and the mating surface with adhesive cleaner. Wipe the tape and the mating surface with a clean, lint free cloth. If the tape is damaged, continue with the replacement procedure.

4. Apply the adhesive foam tape to the back of the emblem/nameplate and press the emblem/nameplate in place.
5. When replacing, remove all adhesive as follows:

• | For body panels, use a 3M™ Scotch Brite molding adhesive remover disk 3M™ P/N 07501 or equivalent.

• | For plastic panels, use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to remove the adhesive.

### Installation Procedure

Important: Apply the emblem/nameplate in an environment that is free from dust or other dirt that could come into contact with the sticky backing. Foreign material may cause improper adhesion.

1. Clean the area where the emblem/nameplate will be installed.

Use a lint free cloth and Varnish Makers and Painters (VMP) naphtha or a (50/50 mixture) by volume of isopropyl alcohol and water in order to clean the area.

2. Dry the area thoroughly.
3. If the location of the emblem/nameplate has not been marked, apply tape and use the following dimensions:

• | The emblem (3) is centered to the high mount stop lamp.

• | Dimension (A) is 17 mm (5/8 in) from the bottom of the high mount stop lamp to the emblem.

4. Heat the mounting surface to approximately 27-41°C (80-105°F).
5. Ensure that the temperature of the emblem/name plate is approximately 29-32°C (85-90°F).
6. Remove the protective liner from the back of the emblem/name plate.
7. Position the emblem/name plate to the location marks and press the emblem/name plate to the mounting surface.
8. Apply equal pressure along the emblem/name plate in order to uniformly bond the item to the mounting surface.
9. Remove the protective tape from the mounting surface.