For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Drums
Brake Drum Inside Diameter New | 225.25 mm | 8.868 in
Brake Drum Maximum Allowable Radial Runout | 0.104 mm | 0.004 in
Brake Drum Maximum Diameter After Refinish | 225.78 mm | 8.889 in
Brake Drum Discard Diameter * | 226.31 mm | 8.909 in
Front Brake Rotors

- Rotor Diameter

278.0 mm

10.944 in

- Lateral Runout

0.04 mm

0.0015 in

- Thickness Variation

0.025 mm

0.001 in

- Rotor Thickness New

26.2 mm

1.031 in

- Minimum Thickness After Refinish

24.9 mm

0.980 in

- Discard Thickness *

24.7 mm

0.972 in

Rear Brake Rotors

- Rotor Diameter

278.0 mm

10.944 in

- Lateral Runout

0.04 mm

0.0015 in

- Thickness Variation

0.025 mm

0.001 in

- Rotor Thickness New

11.0 mm

0.433 in

- Minimum Thickness After Refinish

9.85 mm

0.388 in

- Discard Thickness *

9.0 mm

0.354 in

Front Caliper Bore Diameter | 60.0 mm | 2.36 in
Rear Caliper Bore Diameter | 38.0 mm | 1.50 in
Master Cylinder Bore Diameter | 25.40 mm | 1.00 in
Wheel Cylinder Bore Diameter | 22.20 mm | 0.87 in
* All brake drums and rotors have a discard dimension cast into them. Replace any drum or rotor that does not meet this specification. After refinishing the drum or rotor, replace any drum or rotor that does not meet the maximum diameter or minimum thickness after refinish specification.