For 1990-2009 cars

### Removal Procedure

1. Release the tabs that retain the rear compartment lamp (2) to the rear shelf panel (1). Perform the procedure from inside the rear compartment.
2. Disconnect the electrical connector (3).
3. Remove the bulb from the rear compartment lamp (2).

### Installation Procedure

1. Install the bulb into the rear compartment lamp (2).
2. Connect the electrical connector (3).
3. Press the rear compartment lamp (2) into the rear shelf panel (1) in order to engage the tabs.