For 1990-2009 cars

Table 1: | Fuel Injector Balance Test Example (Actual Results May Vary)

### Circuit Description

The scan tool first energizes the fuel pump and then the injectors for a precise amount of time allowing a measured amount of fuel into the manifold. This causes a drop in system fuel pressure that can be recorded and used to compare each injector.

#### Fuel Injector Balance Test Example (Actual Results May Vary)

Cylinder | 1 | 2 | 3 | 4
--- | --- | --- | --- | ---
1st Reading | 379 kPa (55 psi) | 379 kPa (55 psi) | 379 kPa (55 psi) | 379 kPa (55 psi)
2nd Reading | 280 kPa (41 psi) | 310 kPa (45 psi) | 340 kPa (49 psi) | 317 kPa (46 psi)
Amount of Drop | 99 kPa (14 psi) | 69 kPa (10 psi) | 39 kPa (6 psi) | 62 kPa (9 psi)
Average Range: 47-87 kPa (6.8-12.6 psi) | Replace fuel injector - too much fuel pressure drop | Injector OK | Replace fuel injector - too little fuel pressure drop | Injector OK

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. The engine coolant temperature (ECT) must be below the operating temperature in order to avoid irregular fuel pressure readings due to hot soak fuel boiling.

2. If the pressure drop value for each fuel injector is within 20 kPa (3 psi) of the average pressure drop value, the fuel injectors are flowing properly.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check-Engine Controls? | -- | Go to Step 2 | Go to Diagnostic System Check - Engine Controls
2 | Did you perform the Fuel Injector Coil Test? | -- | Go to Step 3 | Go to Fuel Injector Solenoid Coil Test
3 | Important : Do not perform this test if the ECT is above 94°C (201°F). Observe the ECT parameter with a scan tool. Does the scan tool indicate that the ECT parameter is less than the specified value? | 94°C (201°F) | Go to Step 4 | --
4 | Important: Verify there is adequate fuel in the fuel tank before proceeding with this diagnostic.

1. Turn OFF the ignition.
2. Turn OFF all the accessories.
3. Install the J 34730-1A Fuel Pressure Gage and the fuel pressure gage fitting. Refer to Fuel Pressure Gage Installation and Removal .
4. Turn ON the ignition, with the engine OFF.
5. Command the fuel pump ON with a scan tool.

Important:

• | You may need to command the fuel pump ON a few times in order to obtain the highest possible fuel pressure.

• | Do not start the engine.

6. Observe the J 34730-1A , with the fuel pump commanded ON.

Is the fuel pressure within the specified value?

358-405 kPa (52-59 psi)

Go to Step 5

Go to Fuel System Diagnosis

5 | Important: The fuel pressure may vary slightly when the fuel pump stops operating. After the fuel pump stops operating, the fuel pressure should stabilize and remain constant. Observe the J 34730-1A for 1 minute. Does the fuel pressure drop more than the specified value? | 34 kPa (5 psi) | Go to Fuel System Diagnosis | Go to Step 6
6 |

1. With a scan tool, select the Fuel Injector Balance Test function, within the Special Functions menu.
2. Select an injector to be tested.
3. Press Enter. This will prime the fuel system.
4. Record the fuel pressure indicated by the J 34730-1A after the fuel pressure stabilizes. This is the 1st pressure reading.

Important: Record the fuel pressure value immediately after the fuel injector stops pulsing. The fuel pressure may rise after the fuel injector stops pulsing. Do not record the higher fuel pressure value.

5. Energize the fuel injector by depressing the Pulse Injector button on the scan tool. This will energize the injector and decrease the fuel pressure.
6. Record the fuel pressure indicated by the J 34730-1A after the fuel injector has stopped pulsing. This is the 2nd pressure reading.
7. Press Enter again to bring you back to the Select Injector screen.
8. Repeat for each fuel injector.
9. Subtract the 2nd pressure reading from the 1st pressure reading for one fuel injector. The result is the pressure drop value.
10. Obtain a pressure drop value for each fuel injector.
11. Add all of the individual pressure drop values. This is the total pressure drop.
12. Divide the total pressure drop by the number of fuel injectors. This is the average pressure drop.

Does any fuel injector have a pressure drop value that is either higher than the average pressure drop or lower than the average pressure drop by the specified value?

20 kPa (3 psi)

Go to Step 7

Go to Symptoms - Engine Controls

7 | Clean the fuel injectors. Refer to Fuel Injector Cleaning . Did you complete the action? | -- | Go to Step 8 | --
8 | Operate the vehicle in order to verify the repair. Does a driveability condition still exist? | -- | Go to Symptoms - Engine Controls | System OK