For 1990-2009 cars

### Removal Procedure

1. Turn OFF the ignition.
2. Disconnect the IAT sensor electrical connector.
3. Loosen the air inlet hose clamps.
4. Carefully remove the air inlet hose from the throttle body and MAF sensor.

### Installation Procedure

1. Carefully align the air inlet hose on the throttle body and MAF sensor.
2. Tighten the air inlet hose clamps.
3. Connect the IAT sensor electrical connector.