For 1990-2009 cars

#### Tools Required

J 36660-A Torque Angle Meter

1. Install the front cover gasket. The gasket is reusable and does not require sealer.
2. Inspect the front cover gasket for damage before reusing the gasket.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the upper front cover bolts.

Tighten
Tighten the engine front cover bolts to 12 N·m (106 lb in).

4. Install the engine front cover nuts.

Tighten
Tighten the fasteners to 12 N·m (106 lb in).

5. Lubricate the front oil seal with Chassis Grease GM P/N United States 1051344, GM P/N Canada 993037 or the equivalent.