For 1990-2009 cars

### Removal Procedure

1. Remove the lock pillar lower trim panel. Refer to Lower Pillar Garnish Molding Replacement .
2. Remove the carpet retainer. Refer to Carpet Retainer Replacement in Seats and Carpets.
3. Remove the pillar lower trim panel (1).

Pull firmly and evenly to disengage the retainers.

### Installation Procedure

1. Install the center pillar lower trim panel (1).
2. Install the carpet retainer. Refer to Carpet Retainer Replacement in Seats and Carpets.
3. Install the lock pillar lower trim panel. Refer to Lower Pillar Garnish Molding Replacement .

Ensure the retainers lock into place.