For 1990-2009 cars

#### Tools Required

J 39400-A Halogen Leak Detector

### Removal Procedure

1. For compression-style fittings; use a wrench on the A/C refrigerant component (smaller size) fitting (2), then loosen the A/C refrigerant hose (larger size) fitting (1).
2. For banjo-style fittings; remove the bolt or the nut retaining the A/C refrigerant hose to the A/C refrigerant component.

Important: Cap or tape the open A/C refrigerant hose and the A/C refrigerant component immediately.

3. Disconnect the A/C refrigerant hose from the A/C refrigerant component, discard the O-ring seal and cap or tape the A/C refrigerant hose and the A/C refrigerant component to prevent contamination.

### Installation Procedure

1. Remove the cap or tape from the A/C refrigerant hose and the A/C refrigerant component.
2. Using a lint-free clean, dry cloth, carefully clean the sealing surfaces of the A/C refrigerant hose and the A/C refrigerant component.
3. Lightly coat the new O-ring seal (1) with mineral base 525 viscosity refrigerant oil.

Important: DO NOT allow any of the mineral base 525 viscosity refrigerant oil on the new O-ring seal to enter the refrigerant system.

4. For compression-style fittings; carefully slide the new O-ring seal (1) onto the A/C refrigerant hose until seated.
5. For banjo-style fittings; carefully slide the new O-ring seal (1) onto the A/C refrigerant hose until seated.

Leave a light coating of the refrigerant oil on the A/C refrigerant hose in the area indicated (2) ONLY.

6. Install the A/C refrigerant hose to the A/C refrigerant component.
7. For compression-style fittings; use a wrench on the A/C refrigerant component (smaller size) fitting (2), then tighten the A/C refrigerant hose (larger size) fitting (1) to specification.
8. For banjo-style fittings; install the bolt or the nut retaining the A/C refrigerant hose to the A/C refrigerant component, then tighten to specification.