For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the cruise control cable. Refer to Cruise Control Cable Replacement .
3. Disconnect the electrical connector from the cruise control module assembly.
4. Unclip the hinged retaining strap from the bracket at the top of the module.
5. Remove the cruise control module from the mounting bracket.

### Installation Procedure

1. Install the cruise control module assembly to the mounting bracket.
2. Connect the electrical connector to the module.
3. Install the cruise control cable. Refer to Cruise Control Cable Replacement .
4. Connect the negative battery cable.