For 1990-2009 cars

## Power Steering Return Hose Replacement 2.4L

### Removal Procedure

1. Remove the upper air cleaner assembly. Refer to Air Cleaner Assembly Replacement in Engine Mechanical - 2.4L.
2. Remove the power steering return hose (2) from the power steering pump (1).
3. Raise the vehicle on a hoist. Refer to Lifting and Jacking the Vehicle in General Information.
4. Remove the power steering pressure hose (1) from the power steering gear (3).
5. Remove the power steering return hose (2) from the power steering gear (3).
6. Remove the power steering return hose (2) from the vehicle.

### Installation Procedure

Notice: The inlet and outlet hoses must not be twisted during installation. Do not bend or distort the inlet or outlet hoses to make installation easier. Failure to follow these procedures could result in component damage.

1. Install the power steering return hose (2) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the power steering return hose (2) to the power steering gear (3).

Tighten
Tighten the fitting to 27 N·m (20 lb ft).

3. Install the power steering pressure hose (1) to the power steering gear (3).

Tighten
Tighten the fitting to 27 N·m (20 lb ft).

4. Lower the vehicle.
5. Install the power steering return hose (2) to the power steering pump.
6. Install the upper air cleaner assembly. Refer to Air Cleaner Assembly Replacement in Engine Mechanical - 2.4L.
7. Bleed the power steering system. Refer to Power Steering System Bleeding .

## Power Steering Return Hose Replacement 3.4L

### Removal Procedure

1. Remove the drive belt from the power steering pump pulley. Refer to Drive Belt Replacement in Engine Mechanical - 3.4L.
2. Remove the power steering hose nut (1) and retainer (2).
3. Remove the power steering return hose (3) from the power steering pump (1).
4. Raise the vehicle on a hoist. Refer to Lifting and Jacking the Vehicle in General Information.
5. Remove the power steering return hose (3) from the retainer (6).
6. Remove the power steering return hose (3) from the power steering gear (5).
7. Remove the power steering return hose (3) from the vehicle.

### Installation Procedure

Notice: The inlet and outlet hoses must not be twisted during installation. Do not bend or distort the inlet or outlet hoses to make installation easier. Failure to follow these procedures could result in component damage.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the power steering return hose (3) to the power steering gear (5).

Tighten
Tighten the fitting to 27 N·m (20 lb ft).

2. Install the power steering return hose (3) to the retainer (6).
3. Lower the vehicle.
4. Install the power steering return hose (3) to the power steering pump (1).
5. Install the power steering hose retainer (2) and nut (1).

Tighten
Tighten the nut to 5 N·m (45 lb in).

6. Ensure the the power steering hose has sufficient clearance from the exhaust manifold.
7. Install the drive belt to the power steering pump pulley. Refer to Drive Belt Replacement in Engine Mechanical - 3.4L.
8. Bleed the air from the power steering system. Refer to Power Steering System Bleeding .