For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
DEFINITION: Lead/pull is the deviation of the vehicle from a straight path on a level road with no pressure on the steering wheel.
1 | Did you perform the Vehicle Leads/Pull diagnostic table in Suspension General Diagnosis? | Go to Step 2 | Go to Vehicle Leads/Pulls in Suspension General Diagnosis
2 | Road test the vehicle to verify the complaint. Select a smooth level surface to perform the test Does the condition exist? | Go to Step 3 | System OK
3 |

1. Cross-switch the front tire/wheel assemblies. Refer to Tire and Wheel Removal and Installation .
2. Road test the vehicle on a smooth level surface.

Does the vehicle still lead/pull?

Go to Step 4

System OK

4 | Does the vehicle lead/pull in the opposite direction? | Go to Step 5 | Go to Wheel Alignment Measurement in Wheel Alignment
5 |

1. Cross-switch the left front tire/wheel assembly with the left rear tire/wheel assembly. Refer to Tire and Wheel Removal and Installation .
2. Road test the vehicle on a smooth level surface.

Does the vehicle still lead/pull?

Go to Step 6

Go to Step 7

6 |

1. Cross-switch the right front tire/wheel assembly with the right rear tire/wheel assembly. Refer to Tire and Wheel Removal and Installation .
2. Road test the vehicle on a smooth level surface.

Does the vehicle still lead/pull?

Go to Wheel Alignment Measurement Wheel Alignment Measurement in Wheel Alignment

Go to Step 8

7 | Replace the left rear tire. Refer to Tire Mounting and Dismounting . Is the repair complete? | Go to Step 9 | --
8 | Replace the right rear tire. Refer to Tire Mounting and Dismounting . Is the repair complete? | Go to Step 9 | --
9 | Verify proper vehicle operation. Does the original condition still exist? | Go to Step 1 | System OK