For 1990-2009 cars

### Removal Procedure

1. Disconnect the clutch actuator cylinder line.
2. Remove the transmission. Refer to Transmission Replacement in Manual Transmission - M86/M94 Getrag.
3. Remove the clutch actuator cylinder body bolts.
4. Remove the upper line retainer bolt.
5. Remove the actuator.

### Installation Procedure

1. Lubricate the inside diameter of the bearing with GM P/N 12345777, or equivalent.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the clutch actuator cylinder and the body bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

3. Install the upper line retainer bolt.
4. Install the transmission. Refer to Transmission Replacement in Manual Transmission - M86/M94 Getrag.
5. Connect the clutch actuator cylinder line.
6. Bleed the hydraulic system. Refer to Hydraulic Clutch Bleeding .