For 1990-2009 cars

### Removal Procedure

Important: Do NOT attempt repairs of the lock assembly.

1. Remove the outside door handle assembly. Refer to Door Outside Handle Replacement .
2. Remove the lock cylinder retaining clip in order to remover the lock cylinder (2) from the handle assembly (1).
3. Remove the lock cylinder gasket (4) from the handle assembly (1).

### Installation Procedure

1. Install the lock cylinder gasket (4).
2. Install the lock cylinder (2). Ensure that the retaining clip is locked into position.
3. Install the outside door handle assembly. Refer to Door Outside Handle Replacement .