For 1990-2009 cars

### Removal Procedure

1. Use a small flat-bladed tool on the retainer in order to release the power accessory port housing from the front floor console.
2. Remove the power accessory port housing from the front floor console.
3. Release the electrical connector retainer tabs from the power accessory port.
4. Disconnect the electrical connector from the power accessory port.
5. Remove the retainer and the housing from the bezel, if necessary.

### Installation Procedure

1. Install the retainer and the housing to the bezel, if necessary.
2. Connect the electrical connector to the power accessory port.
3. Position the power accessory port housing to the front floor console.
4. Install the power accessory port housing into the front floor console. Press the housing into place until fully seated.
5. Inspect the power accessory port for proper operation.