For 1990-2009 cars

### Removal Procedure

1. Remove the rocker panel molding screws (2).
2. In order to remove the rocker panel molding (1) complete the following steps:

2.1. | Push upward on the rocker panel molding (1).

2.2. | Disengage the rocker panel molding (1) from the retainers.

3. Remove the rocker panel molding retaining clips.

### Installation Procedure

1. Install the rocker panel molding retaining clips.
2. Snap the rocker panel molding (1) over the retainers.
3. Install the rocker panel molding retaining screws (2). Tighten the screws (2) until the screws are fully driven, seated and not stripped.