For 1990-2009 cars

### Circuit Description

The body control module (BCM) opens the rear compartment when a release input is received from the remote control door lock receiver, or the rear compartment lid release switch.

### Conditions for Running the DTC

The BCM must be commanding the rear compartment lid relay to energize.

### Conditions for Setting the DTC

The BCM detects a short to ground in the rear compartment lid release relay control circuit.

### Action Taken When the DTC Sets

The BCM stores DTC B3267.

### Conditions for Clearing

• | A short to ground is no longer detected in the rear compartment lid release relay control circuit.

• | A history DTC B3267 will clear after 100 consecutive ignition cycles if the condition for the malfunction is no longer present.

• | A scan tool may be used to clear the DTC.

### Diagnostic Aids

• | If the DTC B3267 is a history DTC, the fault may be intermittent. Refer to Testing for Intermittent Conditions and Poor Connections in Wiring Systems.

• | The following conditions may cause an intermittent malfunction to occur:

- | An intermittent short to ground in the rear compartment lid release relay control circuit.

- | The BCM is shorted to ground internally.

### Test Description

The numbers below refer to the step numbers on the diagnostic table.

1. Listen for the rear compartment lid release relay to operate. Repeat the commands as necessary.

2. Verifies that the BCM is providing a ground path to the rear compartment lid release relay.

3. Tests for a short to ground in the rear compartment lid release relay circuit.

Step | Action | Yes | No
--- | --- | --- | ---
Schematic Reference: Body Rear End Schematics
1 | Did you perform the Body Rear End Diagnostic System Check? | Go to Step 2 | Go to Diagnostic System Check - Body Rear End
2 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.
3. With a scan tool, observe the rear compartment lid release relay control parameter in the body control module (BCM) data list.

Does the scan tool display inactive?

Go to Step 3

Go to Step 4

3 |

1. Activate the rear compartment release switch.
2. With the scan tool, observe the rear compartment lid release relay control parameter.

Does the rear compartment lid release relay control parameter change state?

Go to Diagnostic Aids

Go to Step 4

4 |

1. Turn OFF the ignition.
2. Disconnect the rear compartment lid release relay.
3. Turn ON the ignition, with the engine OFF.
4. With a scan tool, observe the rear compartment lid release relay control parameter.

Does the scan tool display inactive?

Go to Step 7

Go to Step 5

5 | Test the signal circuit of the rear compartment lid release relay for an open or short to ground. Refer to Circuit Testing and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 9 | Go to Step 6
6 | Inspect for poor connections at the harness connector of the BCM. Refer to Testing for Intermittent Conditions and Poor Connections and Wiring Repairs in Wiring Systems. Did you find and correct the condition? | Go to Step 9 | Go to Step 8
7 | Replace the rear compartment lid release relay. Did you complete the replacement? | Go to Step 9 | --
8 | Important: Perform the set up procedure for the BCM. Refer to Body Control Module (BCM) Programming/RPO Configuration . Replace the BCM. Refer to Body Control Module Replacement in Body Control System. Did you complete the replacement? | Go to Step 9 | --
9 |

1. Use the scan tool in order to clear the DTCs.
2. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text.

Does the DTC reset?

Go to Step 2

System OK