For 1990-2009 cars

### Removal Procedure

Important: Servicing the IP compartment door lock cylinder will result in a small hole left in the inside top edge of the compartment door. The customer should be advised of this befor servicing the lock cylinder.

1. Open the IP compartment door in order to expose the small dimple located above the lock cylinder.
2. Use a 1/8 inch drill bit in order to drill out the dimple.
3. Insert the key into the lock cylinder.
4. Insert a very small screw driver or pick into the drilled hole and aply pressure to the lock cylinder release tab.
5. Rotate the key in the lock cylinder using the key to pull the lock cylinder from the IP compartment door.

### Installation Procedure

1. Install the lock cylinder into the instrument panel comparement door until fully seated into place.
2. Inspect the operation of the lock cylinder befor closing the IP compartment door.