For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

Caution: This vehicle is equipped with a Supplemental Inflatable Restraint (SIR) System. Failure to follow the correct procedure could cause the following conditions:

• | Air bag deployment

• | Personal injury

• | Unnecessary SIR system repairs

In order to avoid the above conditions, observe the following guidelines:

• | Refer to SIR Component Views in order to determine if you are performing service on or near the SIR components or the SIR wiring.

• | If you are performing service on or near the SIR components or the SIR wiring, disable the SIR system. Refer to Disabling the SIR System.

1. Disconnect the battery ground (negative) cable and the battery (positive) cable from the battery.
2. Remove the battery hold down retainer.
3. Place the underhood junction block aside for access to the battery. Refer to Underhood Fuse Block Replacement .

Important: Do not tip the battery more than 40 degrees during removal.

4. Remove the battery.

### Installation Procedure

Important: Do not tip the battery more than 40 degrees during battery installation.

1. Install the battery to the battery tray.
2. Install the battery hold down retainer.
3. Install the underhood junction block. Refer to Underhood Fuse Block Replacement .

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Connect the battery (positive) cable to the battery.

Tighten
Tighten the battery (positive) cable terminal bolt to 15 N·m (11 lb ft).

5. Connect the battery ground (negative) cable to the battery.

Tighten
Tighten the battery (negative) cable terminal bolt to 15 N·m (11 lb ft).