For 1990-2009 cars

### Removal Procedure

1. Remove the front carpet retainer from the vehicle. Refer to Carpet Retainer Replacement .
2. Pull the front door opening weather-strip (1) loose and remove it from the vehicle.

### Installation Procedure

1. Apply weather-strip adhesive GM P/N 12345096, or equivalent, to the front door opening weather-strip (1).
2. Press the weather-strip (1) onto the front door opening flange.
3. Install the front carpet retainer to the vehicle. Refer to Carpet Retainer Replacement .