For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Control Cable Bracket Bolt/Nut | 10 N·m | 89 lb in
Air Injection Check Valve (with NC1 California Emissions) | 20 N·m | 15 lb ft
Air Injection Check Valve Front Bracket Bolt/Nut (with NC1 California Emissions) | 25 N·m | 18 lb ft
Air Injection Check Valve Bolt/Nut (with NC1 California Emissions) | 10 N·m | 89 lb in
Air Injection Check Valve Pipe Adapter (with NC1 California Emissions) | 30 N·m | 22 lb ft
Air Injection Check Valve Pipe Assembly Bolt | 10 N·m | 89 lb in
Air Injection Check Valve Rear Bracket Bolt/Nut (with NC1 California Emissions) | 25 N·m | 18 lb ft
Air Injection Solenoid Bolt (with NC1 California Emissions) | 10 N·m | 89 lb in
Camshaft Position Sensor Bolt | 10 N·m | 89 lb in
Camshaft Sprocket Bolt | 140 N·m | 103 lb ft
Camshaft Thrust Plate Screw | 10 N·m | 89 lb in
Connecting Rod Bearing Cap Nut

- First Pass

20 N·m

15 lb ft

- Final Pass

75 degrees

Coolant Drain Plug | 19 N·m | 14 lb ft
Coolant Temperature Sensor | 23 N·m | 17 lb ft
Crankshaft Balancer Bolt

- First Pass

70 N·m

52 lb ft

- Final Pass

85 degrees

Crankshaft Main Bearing Cap Bolt/Stud

- First Pass

50 N·m

37 lb ft

- Final Pass

77 degrees

Crankshaft Oil Deflector Nut | 25 N·m | 18 lb ft
Crankshaft Position Sensor Bolt -- Front Cover | 10 N·m | 89 lb in
Crankshaft Position Sensor Stud -- Side of Engine Block | 11 N·m | 98 lb in
Crankshaft Position Sensor Shield Nut | 11 N·m | 98 lb in
Crankshaft Position Sensor Wiring Bracket Bolt | 40 N·m | 30 lb ft
Cylinder Head Bolt

- First Pass

60 N·m

44 lb ft

- Final Pass

95 degrees

Drive Belt Tensioner Bolt | 50 N·m | 37 lb ft
EGR Valve Adapter Pipe to Exhaust Manifold Nut | 25 N·m | 18 lb ft
EGR Valve Pipe to EGR Valve Bolt | 25 N·m | 18 lb ft
Engine Front Cover Bolt

- Large Bolt

55 N·m

41 lb ft

- Medium Bolt

55 N·m

41 lb ft

- Small Bolt

27 N·m

20 lb ft

Engine Mount Strut and A/C Compressor Bracket Bolt | 50 N·m | 37 lb ft
Engine Mount Strut and Lift Bracket Bolt | 70 N·m | 52 lb ft
Engine Mount Strut and Generator Bracket Bolt | 50 N·m | 37 lb ft
Engine Mount Strut and Support Bracket

- Large Bolt

55 N·m

41 lb ft

- Medium Bolt

55 N·m

41 lb ft

- Small Bolt

27 N·m

20 lb ft

Engine Oil Pressure Indicator Switch | 16 N·m | 115 lb in
Engine Wiring Harness Bracket Bolt | 13 N·m | 115 lb in
Exhaust Manifold Heat Shield Bolt | 10 N·m | 89 lb in
Exhaust Manifold Nut | 16 N·m | 12 lb ft
Exhaust Manifold Stud | 18 N·m | 13 lb ft
Flywheel Bolt | 71 N·m | 52 lb ft
Fuel Feed and Return Pipe Bracket Stud | 50 N·m | 37 lb ft
Fuel Feed and Return Pipe Retaining Clip Bolt | 8 N·m | 71 lb in
Fuel Feed and Return Pipe Retaining Clip Nut | 25 N·m | 18 lb ft
Fuel Feed Pipe To Fuel Injector Rail Nut | 17 N·m | 13 lb ft
Fuel Injector Rail Bolt | 10 N·m | 89 lb in
Fuel Pipe Clip Bolt | 8 N·m | 71 lb in
Heated Oxygen Sensor | 42 N·m | 31 lb ft
Heater Inlet Pipe Nut | 25 N·m | 18 lb ft
Heater Inlet Pipe Stud | 50 N·m | 37 lb ft
Ignition Coil Bracket Bolt/Nut/Stud | 25 N·m | 18 lb ft
Intake Manifold Coolant Pipe Bolt | 10 N·m | 89 lb in
Knock Sensor | 19 N·m | 14 lb ft
Lower Intake Manifold Bolt - Center

- First Pass

7 N·m

62 lb in

- Final Pass

13 N·m

115 lb in

Lower Intake Manifold Bolt - Corner

- First Pass

13 N·m

115 lb in

- Final Pass

25 N·m

18 lb ft

MAP Sensor Bolt | 5 N·m | 44 lb in
MAP Sensor Bracket Bolt | 25 N·m | 18 lb ft
Oil Cooler Connector | 50 N·m | 37 lb ft
Oil Cooler Hose Fitting | 19 N·m | 14 lb ft
Oil Cooler Pipe Bracket Bolt | 10 N·m | 89 lb in
Oil Filter | 30 N·m | 22 lb ft
Oil Filter Bypass Plug | 19 N·m | 14 lb ft
Oil Filter Fitting | 39 N·m | 29 lb ft
Oil Gallery Plug -- 1/4 inch | 19 N·m | 14 lb ft
Oil Gallery Plug -- 3/8 inch | 33 N·m | 24 lb ft
Oil Level Indicator Tube Bolt | 25 N·m | 18 lb ft
Oil Level Sensor Bolt | 10 N·m | 89 lb in
Oil Pan Bolt | 25 N·m | 18 lb ft
Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Pan Side Bolt | 50 N·m | 37 lb ft
Oil Pump Cover Bolt | 10 N·m | 89 lb in
Oil Pump Drive Clamp Bolt | 36 N·m | 27 lb ft
Oil Pump Mounting Bolt | 41 N·m | 30 lb ft
Spark Plug

- Spark Plug - Initial Installation

20 N·m

15 lb ft

- Spark Plug - Reinstallation

15 N·m

11 lb ft

Thermostat Bypass Pipe to Engine Front Cover Bolt | 12 N·m | 106 lb in
Thermostat Bypass Pipe to Throttle Body Nut | 25 N·m | 18 lb ft
Throttle Body Bolt/Stud | 25 N·m | 18 lb ft
Timing Chain Dampener Bolt | 21 N·m | 15 lb ft
Upper Intake Manifold Bolt/Stud | 25 N·m | 18 lb ft
Valve Lifter Guide Bolt | 10 N·m | 89 lb in
Valve Rocker Arm Bolt

- First Pass

15 N·m

11 lb ft

- Final Pass

30 degrees

Valve Rocker Arm Cover Bolt | 10 N·m | 89 lb in
Water Outlet Bolt | 25 N·m | 18 lb ft
Water Pump Bolt | 11 N·m | 98 lb in
Water Pump Pulley Bolt | 25 N·m | 18 lb ft

Application | Specification
--- | ---
Metric | English
Camshaft Sprocket Bolt | 140 N·m | 103 lb ft
Crankshaft Balancer Bolt | 103 N·m | 76 lb ft
Drive Belt Tensioner Bolt | 45 N·m | 33 lb ft
Engine Mount Bracket Front Bolt | 102 N·m | 75 lb ft
Engine Mount Bracket Side Bolt | 58 N·m | 43 lb ft
Engine Mount to Body Nut | 66 N·m | 49 lb ft
Engine Mount to Engine Mount Bracket Bolt | 130 N·m | 96 lb ft
Engine Oil Drain Plug | 25 N·m | 18 lb ft
Exhaust Crossover Pipe Bolt | 25 N·m | 18 lb ft
Exhaust Crossover Pipe Heat Shield Bolt | 10 N·m | 89 lb in
Front Cover Bolt (Large) | 47 N·m | 35 lb ft
Front Cover Bolt (Small) | 21 N·m | 15 lb ft
Flywheel Bolt | 83 N·m | 61 lb ft
Lower Intake Manifold Bolt (Diagonal) | 13 N·m | 115 lb in
Lower Intake Manifold Bolt (Vertical) | 13 N·m | 115 lb in
Oil Filter Adapter | 29 N·m | 21 lb ft
Oil Level Indicator Tube Nut | 25 N·m | 18 lb ft
Oil Pan Bolt | 25 N·m | 18 lb ft
Oil Pan Bolt (Side) | 50 N·m | 37 lb ft
Oil Pump Bolt | 41 N·m | 30 lb ft
Oil Pump Drive Bolt | 36 N·m | 27 lb ft
Rocker Arm Bolt

- First Pass

19 N·m

14 lb ft

- Final Pass

30 degrees

Timing Chain Dampener Bolt | 21 N·m | 15 lb ft
Transaxle Bracket Bolt | 75 N·m | 55 lb ft
Upper Intake Manifold Bolt | 25 N·m | 18 lb ft
Valve Lifter Guide Bolt | 10 N·m | 89 lb in
Valve Rocker Arm Cover Bolt | 10 N·m | 89 lb in