For 1990-2009 cars

#### Tools Required

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.
2. Remove the rear seat back. Refer to Rear Seat Back Replacement in Seats.
3. Using J 38778 remove the push in retainers.
4. Remove the shelf trim panel.

### Installation Procedure

1. Position the shelf trim panel over the rear shelf.
2. Install the push-in retainers.
3. Install the rear seat back. Refer to Rear Seat Back Replacement in Seats.
4. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement in Seats.