For 1990-2009 cars

## Front Side Door Window Regulator Replacement Manual

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
3. Remove the front door window. Refer to Front Side Door Window Replacement .
4. Remove the bolts from the front door window regulator.
5. Remove the front door window regulator from the front door.
6. Disconnect the electrical connector.

### Installation Procedure

1. Install the front door window regulator to the front door.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts to the front door window regulator.

Tighten
Tighten the front door window regulator bolts to 10 N·m (89 lb in).

3. Connect the electrical connector.
4. Install the front door window assembly. Refer to Front Side Door Window Replacement .
5. Install the front door water deflector. Refer to Front Side Door Water Deflector Replacement .
6. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .