For 1990-2009 cars

### Removal Procedure

1. Remove the headliner. Refer to Headlining Trim Panel Replacement .
2. Cut the retainer clips off of the rear posts.
3. Remove the overhead console (1) from the headliner.

### Installation Procedure

1. Position the overhead console (1) into the headliner.
2. Push two new retainer clips onto the console rear attaching posts.
3. Install the headliner. Refer to Headlining Trim Panel Replacement .