For 1990-2009 cars

### Removal Procedure

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .
2. Disconnect the fuel pressure regulator vacuum line.
3. Remove the fuel pressure regulator attaching screw.
4. Using a shop towel to catch any spilled fuel, lift and twist the fuel pressure regulator in order to remove the fuel pressure regulator from the fuel rail.
5. Remove the retainer and spacer bracket from the rail and discard.
6. Remove the fuel pressure regulator from the engine fuel return pipe.
7. Remove the fuel pressure regulator inlet O-ring and the fuel return pipe O-ring and discard.

### Installation Procedure

Caution: Connect the fuel return line before tightening the regulator attaching screw in order to prevent the regulator from rotating. Rotation of the regulator could damage the retainer and spacer bracket and lead to a fuel leak at the regulator inlet.

Notice:

• | Do not use compressed air in order to test or clean a fuel pressure regulator as damage to the fuel pressure regulator may result.

• | Clean the fuel pressure regulator filter screen with gasoline if necessary.

• | Do not immerse the fuel pressure regulator in a solvent bath in order to prevent damage to the fuel pressure regulator.

1. Inspect the filter screen for contamination. If contaminated, replace the fuel pressure regulator.
2. Lubricate the new pressure regulator inlet O-ring with clean engine oil and install on the regulator inlet.
3. Lubricate the new fuel return pipe O-ring with clean engine oil.
4. Install the fuel return pipe O-ring.
5. Connect the fuel return pipe to the regulator.
6. Install the new retainer and spacer bracket into the slot on the fuel rail.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

7. Install the pressure regulator to the fuel rail.

Tighten
Tighten the fuel return pipe fitting to 17 N·m (13 lb ft).

8. Connect the fuel pressure regulator vacuum line.
9. Install the pressure regulator attaching screw.

Tighten
Tighten the pressure regulator attaching screw to 8.5 N·m (75 lb in).

10. Inspect and verify that the retainer and spacer bracket is engaged in the slots in the fuel rail. Grasp and pull on the regulator to ensure that the regulator is properly seated.
11. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection in Engine Electrical.
12. Inspect the fuel leaks using the following procedures:

12.1. | Turn ON the ignition, with the engine OFF for 2 seconds.

12.2. | Turn OFF the ignition for 10 seconds.

12.3. | Turn ON the ignition, with the engine OFF.

12.4. | Inspect for fuel leaks.