For 1990-2009 cars

### Removal Procedure

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief .
2. Drain the fuel tank. Refer to Fuel Tank Draining .
3. Raise the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
4. Disconnect the quick-connect fitting at the fuel filter. Refer to Plastic Collar Quick Connect Fitting Service .
5. Disconnect the fuel return pipe quick connect fitting. Refer to Plastic Collar Quick Connect Fitting Service .
6. Remove the rubber exhaust hangers. Allow the exhaust system to rest on the rear axle.
7. Remove the exhaust heat shield.
8. Loosen the fuel filler hose clamp at the fuel tank.
9. Disconnect the fuel filler hose from the fuel tank.
10. Disconnect the evaporative emission (EVAP) vapor pipe from the EVAP canister.
11. Disconnect the electrical harness from the multi-way rear body connector and fuel strap.
12. With the aid of an assistant, support the fuel tank (1).
13. Disconnect the fuel tank retaining straps.
14. Lower the fuel tank.
15. Remove the fuel sender assembly from the tank. Refer to Fuel Sender Assembly Replacement .

### Installation Procedure

1. Install the fuel sender assembly to the fuel tank. Refer to Fuel Sender Assembly Replacement .
2. With the aid of an assistant, raise the fuel tank (1) to the vehicle.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the fuel tank retaining straps.

Tighten
Tighten the strap bolts to 35 N·m (26 lb ft).

4. Connect the wiring harness into the multi-way rear body connector.
5. Connect the EVAP vapor pipe to the EVAP canister.
6. Connect the fuel filler hose to the fuel tank.

Tighten
Tighten the fuel filler hose clamp to 3 N·m (27 lb in).

7. Install the rubber exhaust hangers.
8. Install the exhaust heat shield.

Tighten

• | Tighten the exhaust shield bolt to 2 N·m (18 lb in).

• | Tighten the exhaust shield nuts to 1 N·m (9 lb in).

9. Connect the fuel return pipe and fuel filter quick-connect fittings. Refer to Plastic Collar Quick Connect Fitting Service .
10. Lower the vehicle.
11. Refill the fuel tank.
12. Install the fuel filler cap.
13. Connect the negative battery cable.
14. Inspect for fuel leaks.

14.1. | Turn ON the ignition for 2 seconds.

14.2. | Turn OFF the ignition for 10 seconds.

14.3. | Turn ON the ignition.

14.4. | Inspect for fuel leaks.