For 1990-2009 cars

#### Tools Required

• | J 8062 Valve Spring Compressor

• | J 36017 Valve Guide Seal Remover

1. Remove the coolant outlet.
2. Remove the O-ring.
3. Remove valve train components.

Important: Ensure that the valve train components are kept together and identified in order for proper re-installation in their original position.

4. Compress the valve spring, using the J 8062 .
5. Remove the valve keys.
6. Slowly release the J 8062 from the valve spring assembly.
7. Remove the valve retainer.
8. Remove the valve spring.
9. Remove the valve spring seat (exhaust only).

Notice: Do not damage the valve guide. Remove any burrs that have formed at the key groove by chamfering the valve stem with an oil stone or a file.

10. Remove the valve seal, using the J 36017 .
11. Remove the valve rotator (intake only).
12. Remove the valve.
13. Remove the remaining valves.