For 1990-2009 cars

### Removal Procedure

1. Position the front to the most rearward position.
2. Remove the seat adjuster release handle retaining clips.
3. Remove the seat adjuster release handle from the seat track studs.

### Installation Procedure

1. Install the seat adjuster release handle to the seat track studs.
2. Install the seat adjuster release handle retaining clips, pressing into place until fully seated.
3. Position the front to the original position.