For 1990-2009 cars

## Radiator Inlet Hose Replacement 2.2L

#### Tools Required

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the cooling system. Refer to Cooling System Draining and Filling .
2. Use theJ 38185 in order to reposition the outlet hose clamp from the cylinder head (2).
3. Remove the outlet hose from the cylinder head.
4. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
5. Use theJ 38185 in order to reposition the outlet hose clamp from the radiator.
6. Remove the outlet hose (2) from the radiator.

### Installation Procedure

1. Install the outlet hose (2) to the radiator.
2. Use theJ 38185 in order to reposition the outlet hose to the radiator.
3. Lower the vehicle.
4. Install the outlet hose to the cylinder head (2).
5. Use theJ 38185 in order to position the outlet hose to the cylinder head.
6. Fill the cooling system. Refer to Cooling System Draining and Filling .

## Radiator Inlet Hose Replacement LA1

#### Tools Required

J 38185 Hose Clamp Pliers

### Removal Procedure

1. Drain the cooling system to a level below the hose being removed. Refer to Cooling System Draining and Filling .
2. Use the J 38185 in order to reposition the radiator inlet hose clamp (1) at the water outlet.
3. Remove the radiator inlet hose from the water outlet.
4. Use the J 38185 in order to reposition the inlet hose clamp at the radiator.
5. Remove the radiator inlet hose (2) from the radiator .

### Installation Procedure

1. Install the radiator inlet hose (2) to the radiator.
2. Use the J 38185 in order to reposition the inlet hose clamp at the radiator.
3. Install the radiator inlet hose (2) to the water outlet.
4. Use the J 38185 in order to reposition the inlet hose clamp (1) to the water outlet.
5. Fill the cooling system. Refer to Cooling System Draining and Filling .